<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="30.3966875" y1="14.1914875" x2="30.3966875" y2="1.4914875" width="0" layer="20"/>
<wire x1="30.3966875" y1="1.4914875" x2="29.1266875" y2="0.2214875" width="0" layer="20"/>
<wire x1="29.1266875" y1="0.2214875" x2="25.6341875" y2="0.2214875" width="0" layer="20"/>
<wire x1="25.6341875" y1="0.2214875" x2="24.6816875" y2="-0.7310125" width="0" layer="20"/>
<wire x1="24.6816875" y1="-0.7310125" x2="15.7916875" y2="-0.7310125" width="0" layer="20"/>
<wire x1="12.6166875" y1="2.4439875" x2="12.6166875" y2="13.2389875" width="0" layer="20"/>
<wire x1="15.7916875" y1="16.4139875" x2="24.6816875" y2="16.4139875" width="0" layer="20"/>
<wire x1="24.6816875" y1="16.4139875" x2="25.6341875" y2="15.4614875" width="0" layer="20"/>
<wire x1="25.6341875" y1="15.4614875" x2="29.1266875" y2="15.4614875" width="0" layer="20"/>
<wire x1="29.1266875" y1="15.4614875" x2="30.3966875" y2="14.1914875" width="0" layer="20"/>
<wire x1="12.6166875" y1="13.2389875" x2="15.7916875" y2="16.4139875" width="0" layer="20" curve="-90"/>
<wire x1="12.6166875" y1="2.4439875" x2="15.7916875" y2="-0.7310125" width="0" layer="20" curve="90"/>
<text>Z-Probe V1.0</text>
<text>RUMBA</text>
<text>RUMBA</text>
<text>MELZI</text>
<text>MELZI</text>
<text>MELZI</text>
<text>RAMPS</text>
<text>RUMBA</text>
<text>RAMPS</text>
<text>www.active3d.co.uk</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_3">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE05-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MELZI_GND" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="MELZI_GND1" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="BSS138">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="RUMBA_GND" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SENSOR" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lsta" package="FE05-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SENSOR" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="RUMBA_GND" pad="2"/>
<contactref element="MELZI_GND" pad="2"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="SJ1" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="MELZI_GND1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="SENSOR" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="SIGNAL">
<contactref element="Q1" pad="3"/>
<contactref element="LED1" pad="C"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="RUMBA_GND" pad="1"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="MELZI_GND" pad="1"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="SJ1" pad="2"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="SJ2" pad="2"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="MELZI_GND1" pad="2"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="2.8V">
<contactref element="SENSOR" pad="1"/>
<contactref element="SENSOR" pad="2"/>
<contactref element="SJ2" pad="3"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
